C.4. Partitions with enforced heat transfer coefficient <br>

C.4. Partitions with enforced heat transfer coefficient

Error: Elevated floor does not have an aerial layer

Error occurring, when the aerial layer has not been declared for elevated floor.

Error: Unacceptable presence of element of type: Partition layer

Error concerning entering of aerial layer as first from internal side or as last from external side of layer.

Warning: Condensation occurring inside the partition or on its internal side

Message informing about occurring of water vapour condensation inside the defined partition or on its internal surface.