C.8. Partitions<br>

C.8. Partitions

Error: Partition can not be assigned to two compartments

Error occurring during assigning of internal partition to two compartments.

Warning: Errors in partition definition

This warning is generated, when in compartment will be declared partition, which has been declared with errors. Go to “Partitions definition” and correct there errors occurring in partition.

Warning: Internal partition used between compartments on various storeys

Message concerns situation, where internal wall has been assigned to compartment located on another storey.

Internal ceiling used between compartments on the same storey

Message displayed in case of using of internal ceiling between compartments belonging to the same storey

Heat flow direction differs from declared one in partition construction

Message concerns a situation, where there is a difference between heat flow direction declared for specific partition in “Partition definitions” and resulting from their application in building structure. Message concerns such partitions as e.g. windows, internal doors.

Warning: Internal ceiling used between not adjacent storeys

Message concerns a situation, where the internal ceiling has been used between not adjacent storeys.