5.3.4. Setting up of compartment losses<br>

### 5.3.4. Setting up of compartment losses

For each group of results there is an information concerning project name, theme of displayed results and project data. Compartments data have been presented in tabular form.

No. |  |
Number of compartment | number of compartment and its description. This column also contains the value of temperature in compartment, area and cubic capacity |
ΦT,e |  |
ΦT | heat loss by penetration | [W]
ΦV,min | heat loss for minimal ventilation | [W]
ΦV,inf | heat loss for infiltration | [W]
ΦV,su | heat loss resulting from mechanical air blow with lower temperature than the temperature in compartment | [W]
ΦV,mech,inf | heat loss as a result of excess of air exhausted mechanically from compartment | [W]
ΦNetto | sum of heat losses by penetration and ventilation | [W]
ΦRH | additional heat loss resulting from temporary temperature reduction in compartment | [W]
Φi | compartment heat demand | [W]