C.1. General data and results<br>

C.1. General data and results

Error: Exceeded maximal number of storeys (max=3) for simplified method of heat losses calculation

Error is displayed in simplified method of heat loss calculation in case of inserting into the building structure the number of storeys exceeding 3.

Error: Impossible to determine automatically the heat capacity, because the partitions from outside the partition definition on the level of construction has been used

Error informing about lack of possibility of calculation of heat capacity by the program because of lack of data. Appears after declaring of partition directly in building structure.

Error: Lack of data in catalogue required for calculations of seasonal energy demand

Message informing about lack of data in catalogue, required for calculations of seasonal energy demand in the building. Selected climatic data can be not completed with values required for these calculations.

Error: Lack of relation storey in project

Error displaying in case of not declaring the relation storey in building structure

Error: Building depression too big

Message displayed in case of declaring of building depression over the value resulting from diagram

Warning: Internal graphical partitions have been hidden , which must be included in calculations of ‘%s’. Switch on the option ‘%s’.

Message displayed in case of selecting of option ‘Hide non-cooling partitions” and data of which concerning heat capacity are required for calculations of temporary temperature reduction in compartments.

Error: Too low temperature on heaters supply

This error will appear, when the value of heaters supply temperature from beyond the lower limit will be given.

Warning: Given external temperature differs from the temperature from climatic data

Message appearing after entering the value of external air temperature and then after connecting of calculation of seasonal energy demand and selecting the meteorological and actinometrical station from the catalogue of climatic data.

Warning: Average given annual outer temperature is different than temperature from climatic data

Message appearing, if the User will give the value of average annual outer temperature different than the value of this temperature included in climatic data.

Error: Meteorological station – not completed

Error appearing, when the meteorological station will not be selected from the catalogue of climatic data. It is necessary to select a location from the catalogue of climatic data, the meteorological station will be assigned automatically.

Error: Actinometrical station – not completed

Error appearing, when the actinometrical station will not be selected from the catalogue of climatic data. It is necessary to select a location from the catalogue of climatic data, the actinometrical station will be assigned automatically.

Error: Default type of heater – not completed

Error informing about lack of declaration of default type of heater among heaters available in heaters catalogue, after declaring of heaters selection in compartment in „Heaters selection data”.

Error: Too low number of storey with heat source

Error appearing after declaring of too low number of storeys with heat source in relation to the number of storeys in building. Such message appears extremely rare, because storeys are numbered from 0 up. Only after declaring in field a function, which would give an negative number, this message will appear.

Error: Too high number of storey with heat source

Error appearing after declaring of too high number of storeys with heat source in relation to the number of storeys in building.