C.9. Heaters and heat distribution <br>

C.9. Heaters and heat distribution

Warning: No heater selected

Message informing, that not any heater has been selected in compartment. It can be more reasons for such situation, for example lack of heater of selected type, with required thermal power.

Error: Power of enforced heaters exceeds required power of heaters in compartment

Message concerns a situation, in which the power of heaters exceeding the required heat loss to be covered by heating Qexc. has been declared in heaters selection table.

Error: Power of enforced heaters does not ensure required power of heaters in compartment

This message concerns a situation, in which the power of heaters not ensuring required power of heaters to be covered by heating Qexc./Φexc. has been declared in heaters selection table.

Error: Incorrect manual distribution Q

Error occurring, when in table of heat distribution into various types of heating the sum of shares of various types of heating will exceed the value of heat losses to be covered by heating Qexc./ Φexc..

Error: Summary distribution Q different from declared one

Message informing about discrepancy of value of summary heat distribution, which will be described on the tab „Heat distribution” with the value of declared heat distribution in field „Qdistr” („%Qdistr) / “Φdistr” (“%Φdistr”).

Error: Errors in element inserted in graphical editor – check warnings

Message informing about errors occurring in an element, which has been loaded from Instal-therm program. Check the displayed warnings and correct the element in Instal-therm program.