C.2. Partitions definitions<br>

C.2. Partitions definitions

Warning: Incorrect name

Message appearing, when the User has not entered the name of defined partition.

Error: Duplicated name

Error occurring after entering of the same name for several partitions.

Error: Partition being part of inhomogeneous partition does not exist

Message appearing, if an element of inhomogeneous partition which has been declared in “Partition definitions” has been removed.

Error: Inhomogeneous partition can not be an element of inhomogeneous partition

Message concerns a situation, where an element of inhomogeneous partition is an inhomogeneous partition

Error: Share of inhomogeneous partition element from outside the scope (0-100%)

Message appearing, if the declared share of component element in area of inhomogeneous partition is not included in determined scope (0-100%), e.g. if an letter will be entered.

Error: Sum of shares of inhomogeneous compartment elements should be equal to 100%

Message appearing, if the sum of shares of individual component elements in area of inhomogeneous partition is > or < 100%.

Error: Name of share of inhomogeneous partition is incorrect

Error: Type of partition being an element of inhomogeneous partition is incorrect

Message concerns situation, in which there is no compatibility between types of elements of inhomogeneous partition and the type of inhomogeneous partition.

Error: Inhomogeneous partition can not contain itself as the share

Message appearing after declaring of component element with the same name as inhomogeneous partition. Entering the name a partition will be selected.

Hint: Partition appears as an element of inhomogeneous partition more than once

Program hint informing the User about multiple using of the same partition as an element of inhomogeneous partition.

Hint: Elevated floor has been used in compartment with depression greater than 0

Message informing about using of elevated floor in compartment which is depressed under the ground level.

Error: Not elevated floor has an aerial layer

Message concerns the case when in floor not declared as “Elevated” an aerial layer has been declared in layers table.