B.4. Heaters selection<br>

B.4. Heaters selection

A basis for heater selection is the reduced heat loss taking into account the heat loss division from other compartments and into various methods of heating. After taking into consideration of all multipliers declared in data, increasing the heater’s surface, the program selects a heater from indicated catalogue.

Multipliers increasing the surface of heater are taken into account on the basis of declared type of housing and heater location. The multiplier taking into consideration divergences between designed system and its real execution will be taken into account by the program, if in „Heaters selection data” its application will be declared. The multiplier taking into consideration the cooling down of water in pipes is accepted on the basis of declared storey, on which a heater is located and the storey, on which the heat source is located, that means on the basis of number of storeys dividing them.